Alitherm 800 Windows

Kitemark 81543 (Pas24-2012 Security, BS6375 Part 1 & 3 Weather)

Designed for use as fixed lights and open out windows, internally or externally beaded, for domestic and light commercial applications.

Thermal breaks are formed with polyamide strips PA 6.6 25 reinforced with glass fibre, fitted between aluminium extrusions. All profiles are extruded from aluminium alloy 6060/6063 T5/T6 and comply with the recommendations of BS EN 12020-2; 2001/BS 755-9: 2001. Profiles can be Electrostatic powder coat finished in a range of RAL colours to APA Qualicoat guidelines with the option of BI-colour, different internal and external colours. Other finishes include anodised in satin with EWAA/EURAS-Qualanod quality label. All opening vents are hung on concealed stainless steel variable angle friction stays and fitted with cockspur/espagnolette/espagnolette shoot bolt locking mechanisms.

Glazing conforms to the requirements of BS 6262 and Part ‘N’ of the Building Regulations for both thickness and type.

Internal or external beads and gaskets will accommodate 24mm, 28mm and 32mm units.

Windows are manufactured according to customer requirements from a range of standard profiles and are designed to incorporate a range of vent openings and various options, therefore it is advisable to contact Smart Systems technical design department early in the design process.

Product tested to BS6375: Part 1 & 2 Weathertightness classification:

Air Permeability – Class 3 600Pa

Watertightness – Class E1050Pa

Wind resistance – Class A5 2000Pa

Windows are manufactured to the required design to within the following maximum limitations (subject to location).

Side opening – Max width 700mm, and maximum height 1400mm. Maximum weight 28kg

Top Opening – Max height 1300mm and max width 1400mm. Maximum weight 40kg.

Subject to agreement it is possible to exceed these limitations depending on design criteria, contact Smart Systems Technical Department for details.

Consult Smart Systems Ltd technical literature for details. Smart Systems Ltd can also provide design and specification guidance and it is recommended that they are consulted early in the design process.

**Manufacturer**: Smart Systems Ltd. Arnolds Way, Yatton, North Somerset BS49 4QN.  
Tel: 01934 876100. Fax: 01934 835169.  
Email: [sales@smartsystems.co.uk](mailto:sales@smartsystems.co.uk) Web: [www.smartsystems.co.uk](http://www.smartsystems.co.uk)

**Product reference**: Alitherm 800 Series Windows

**Materials**: All profiles are extruded from aluminium alloy 6060/6063 T5/T6 and comply with the recommendations of BS EN 12020-2; 2001/BS 755-9: 2001. Thermal breaks are formed with polyamide strips PA 6.6 25 reinforced with glass fibre sections capable of withstanding temperatures up to 200°C for over painting.

**Performance**: Product tested to BS6375: Part 1. (Air Permeability – Class 3 600Pa. Watertightness – Class E1050Pa. Wind resistance – Class A5 2000Pa)

**Exposure**: Design Wind Pressure **TBA**

**Thermal**: All windows, in conjunction with a suitable glazing specification, to achieve an average project U-value to meet the current requirements of the approved Building Regulation Document L1/L2 for England and Wales. Target window U-value **TBA**

**Structure**: All structural profiles to be designed to meet CWCT guidelines.

**Construction**: All windows shall be manufactured, installed and glazed in strict accordance with Smart Systems instructions and guidelines as set down in the appropriate technical literature, details and specifications.  
Minimum depth of outer frame sections shall be 61mm incorporating two 35mm polyamide thermal break sections within the window profiles. All outer frame and vent members to be 45° mitred corner construction, reinforced by means of extruded aluminium cleats and stainless steel corner braces. All corner joints to be secured by gluing & crimping. All mullions and transoms to be cut/shaped and secured using either stainless steel screws driven into integral screw ports within the sections or cleats. All joints to be sealed during construction using suitable ‘small gap’ sealant. The windows to incorporate an internal pressure equalized drainage system with concealed down drainage through a sub sill or frontal drainage with snap on cover caps.

**Finish as Delivered:** Internal Colour: **TBA** External Colour: **TBA**

**Glazing details**: Glazing shall be site glazed as section L40.  
Windows shall be double glazed and externally or internally beaded. (Refer to contract specification)  
Unit thickness. Overall thickness of 24, 28 or 32mm depending on profiles selected. All windows to be dry glazed using shuffle extruded aluminium beads and EPDM extruded gaskets.

**Ironmongery / Accessories:** TBA

**Fixing**: All fixings to be in strict accordance with the relevant British Standards, including BS 6262 and BS8213 Part 4 Part 4 2007, and shall ensure the window is retained securely within the opening without incurring any damage or distortion to the window frame. Generally, fixings to be positioned 150mm from each corner and each mullion/transom and at centres not exceeding 600mm. Fixing lugs/straps only to be used where they can be suitably concealed to approval. All Fixing of windows to the supporting structure to be achieved using a suitable lug and/or frame anchor fixing method capable of accommodating all applicable loads, deflection, tolerances and expansion expected on site.