Visoglide Plus Patio Door - kitemark km530838 (inc PAS24: 2012 for slide-only)

Designed for use as a sliding door, internally beaded, with triple track options, for domestic and light commercial applications. Doors can be either Slide only, or Lift and Slide configuration.

Door and door frames are extruded from aluminium alloy 6060/6063 T5/T6 and comply with the recommendations of BS EN 12020-2; 2001/BS 755-9: 2001. Profiles can be Electrostatic powder coat finished in a range of RAL colours to APA Qualicoat guidelines with the option of BI-colour, different internal and external colours. Other finishes include anodised in satin with EWAA/EURAS-Qualanod quality label. All doors are sliding on stainless steel rollers with max weight per panel of 250kgs and fitted with multi-point locking mechanisms or key-operated vertical shoot bolts. Lift and slide max weight per panel is 200kgs with multi-point locking.

Glazing conforms to the requirements of BS 6262 and Part ‘N’ of the Building Regulations for both thickness and type.

Internal or external bead and gaskets will accommodate 28, 29, 30, 36, 37 or 38mm units.

Product tested to BS6375: Part 1. Weathertightness classification:

Air Permeability – Class 3 600Pa

Watertightness – Class 7A 300Pa

Wind resistance – Class AE 2400Pa

Doors are manufactured according to customer requirements from a range of standard profiles and are designed to incorporate a range of options, therefore it is advisable to contact Smart Systems technical design department early in the design process.

Doors are manufactured to the required design to within the following maximum limitations (subject to location).

Max height 2500mm Width 7000mm (Subject to Wind Load calculations)

Max weight 250kgs Slide only, 200kgs Lift and Slide.

Subject to agreement it is possible to exceed these limitations depending on design criteria, contact Smart Systems Technical Department for details.

Consult Smart Systems Ltd technical literature for details. Smart Systems Ltd can also provide design and specification guidance and it is recommended that they are consulted early in the design process.

**Manufacturer**: Smart Systems Ltd. Arnolds Way, Yatton, North Somerset BS49 4QN.  
Tel: 01934 876100. Fax: 01934 835169.  
Email: [sales@smartsystems.co.uk](mailto:sales@smartsystems.co.uk) Web: [www.smartsystems.co.uk](http://www.smartsystems.co.uk)

**Product reference**: Visoglide Plus

**Materials**: All profiles are extruded from aluminium alloy 6060/6063 T5/T6 and comply with the recommendations of BS EN 12020-2; 2001/BS 755-9: 2001. Thermal breaks are formed with polyamide strips PA 6.6 25 reinforced with glass fibre sections capable of withstanding temperatures up to 200°C for over painting.

**Exposure**: Design Wind Pressure TBA

**Thermal**: All doors, in conjunction with a suitable glazing specification, to achieve an average project U-value to meet the current requirements of the approved Building Regulation Document L1/L2 for England and Wales. Target window U-value TBA.

**Construction**: All doorsets shall be manufactured, installed and glazed in strict accordance with Smart Systems instructions and guidelines as set down in the appropriate technical literature, details and specifications. Depth of outer frame sections shall be 99 or 116mm for two track, or 165.5 or 182.5 for three track. All outer frame and door members to be 45° mitred corner construction, reinforced by means of extruded aluminium cleats and stainless steel corner braces. All corner joints to be secured by gluing and mechanical corner Cleats. All mullions and transoms to be cut/shaped and secured using stainless steel screws driven into integral screw ports within the sections or with mechanical Cleats. All joints to be sealed during construction using suitable ‘small gap’ sealant. It is recommended that the door system be drained and ventilated in accordance with Smart Systems Technical Manual.

**Finish as Delivered:** Internal Colour: TBA External Colour: TBA

**Glazing details**: Glazing shall be site glazed as section L40. Doors shall be glazed internally square beaded. Unit thickness. Overall thickness of 28, 29, 30, 36, 37 or 38mm. All doors to be dry glazed using shuffle extruded aluminium beads and EPDM extruded gaskets.

**Ironmongery / Accessories: For PAS24 : 2012 COMPLIANCE REFER TO PAS24 HARDWARE SCHEDULE**

**Fixing**: All fixings to be in strict accordance with the relevant British Standards, including BS 6262 and BS8213 Part 4: 2007, and shall ensure the door frame is retained securely within the opening without incurring any damage or distortion to the door frame. Generally, fixings to be positioned 150mm from each corner and each mullion/transom and at centres not exceeding 600mm. Fixing lugs/straps only to be used where they can be suitably concealed to approval. All Fixing of door frames to the supporting structure to be achieved using a suitable lug and/or frame anchor fixing method capable of accommodating all applicable loads, deflection, tolerances and expansion expected on site.